**D4330**

**Features:**· 33 detection zones  
· 7"LCD HD display interface  
· Remote control  
· Simple installation and use  
· In and out count  
· Excellent anti-interference ability and stability  
· Each zone has 300 adjustable sensitivity level  
· Supports various language interface customization  
· Higher accuracy and verifcation speed  
· Pass count and Alarm count memory function

**Parameter**

|  |  |
| --- | --- |
| Input voltage | 15V |
| Working temperature | -20℃～65℃ |
| External Dimensions | 2220mm(H)\*930mm(W)\*760mm(D) |
| Channel Dimensions | 2010mm(H)\*760mm(W)\*760mm(D) |
| Package Dimensions | 2300mm(H)\*335mm(W)\*800mm(D) |
| Gross weight | 70kg |