**ES-32B11J**

Parameter

|  |  |
| --- | --- |
| **Camera** |   |
| Model | ES-32B11J |
| Image Sensor | 1/2.9” 2MP Sensor |
| Scanning System | Progressive |
| Min. Illumination | 0.1Lux/F2.4 (color)0 Lux with IR on |
| Effective Pixels | 1920(H)\* 1080(V)  |
| S/N Ratio | More than 52dB |
| IR Distance | 10~20m |
| IR LED No. | 10 |
| **Lens** |   |
| Focal Length | 2.8mm |
| Aperture  | F2.4 |
| FOV | 92° |
| **Video** |   |
| Video Output | AHD/TVI/CVI/CVBS |
| Resolution | 25/30fps@1080P |
| OSD Menu | Supported |
| BLC | N/A |
| WDR  | DWDR |
| AGC | Supported |
| Day/Night | Auto(ICR)/Manual |
| White Balance | Supported |
| Noise Reduction | 2D DNR  |
| **General** |   |
| Working Temperature | -30°C~+60°C |
| Working Humidity | 10~90% |
| Power Supply | DC12V±10% |
| Power Consumption | ＜3.2W(IR off) |
| Dimensions | Φ92x78mm |
| Net Weight | 0.13KG |
| Gross Weight | 0.2KG |