TF1700

F1700 is one of the world’s smallest Ethernet connection-based fingerprint terminals, used for access control and time attendance features, with IP65 waterproof housing.  
With its IP65 rated rugged waterproof and dustproof structure, TF1700 offers extra durability in harsh conditions such as outdoor environments. It is specially designed for standalone applications such as house, office, shop, garage, factory and others.  
The 2013 version of TF1700 is equipped with a sensor cover to protect the optical reader and updated with new firmware that supports ZKAccess3.5 management software which has versatile features and powerful functions.

 .**Features**

* Full Access Control Features
* Slim and Elegant Design
* Fast and Accurate Fingerprint Algorithm
* Easy Operation and Management

**Parameter**

|  |  |
| --- | --- |
| Fingerprint Sensor | Infrared detection fingerprint sensor |
| Algorithm Version | ZK Finger VX10.0 |
| Communication | TCP/IP, RS485, USB Host |
| Fingerprint Capacity | 3,000 Fingerprints(8,000 Optional) |
| Card Capacity | 10,000 Cards |
| Log Capacity | 50,000 Transactions |
| RF Card | EM(standard)/Mifare(optional) |
| Authentication | Finger/PIN/Card |
| Wiegand Signal | Wiegand input&output |
| Ingress Protection Rate | IP65 |
| Display | 128 x 64 OLED |
| Keypad | 3 x 5 keypads & doorbell |
| Sound and Interface | Buzzer and multi-color LED |
| Operating Voltage | 12VDC 3A |
| Operating Temperature | -10 °C~50 °C (14°F ~ 122°F) |
| Dimension | 62.5mm×185mm×41.5mm (W×H×D) |